STERILE IPA 70% in WFI

2 x 5l capped bottles per case.

item no. 0038

AGMA STERILE ipa 70% in WFI is a proven means for continual disinfection within cleanrooms.

AGMA STERILE ipa 70% in wfi is commonly used in cleanroom facilities including in hospital or pharmaceutical environments. AGMA STERILE ipa 70% in WFI is a reliable, cost-effective means of routine disinfection. ideal for use with sterile dry mops.

As well as a proven disinfectant, ipa 70% evaporates fully leaving no residues.

* Manufactured in ISO Class 5 Cleanroom
* 0.2 micron filtered
* Individually double bagged
* Gamma irradiated for sterility
* High Purity WFI quality WATER
* Endotoxin < 0.25UI/ml
* Fully traceability with supporting analysis.
* 2-year shelf life.
* Efficacy validated externally

Direction for Use:

AGMA ipa 70% is manufactured for use on cleanroom ceilings, walls, floors and equipment hard surfaces.

Ensure complete wetting of the surface. Do not use to treat surfaces that are particularly sensitive to alcohol such as acrylic glass. Always close container after use.

 Use Biocides Safely. Always read the label and product information.

The information contained in this data sheet is accurate to the best of our knowledge and belief. No warranty is, however, given or implied.Consult Agma Ltd concerning all non-standard applications.

Issue No. 1-03/23